For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.

• | Disconnect the negative cable.

• | Disconnect the positive cable.

2. Remove the battery holder (1).

Remove the bolt.

3. Remove the battery.

### Installation Procedure

1. Install the battery.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the battery holder.

Tighten
Tighten the bolt to 7 N·m (62 lb in).

3. Connect the battery.

• | Connect the positive cable.

• | Connect the negative cable.

4. For programming procedures, refer to Control Module References.