For 1990-2009 cars

### Removal Procedure

1. Remove the windshield trim seal (1).
2. Remove the wiper arms (2).

• | Remove the 2 covers.

• | Remove the 2 nuts.

• | Remove the 2 washers.

• | Remove the 2 windshield wiper arms from the shaft.

3. Remove the windshield air inlet screen (1).

• | Lift the windshield air inlet screen at the front.

| Important: Carefully release the clips from the air inlet screen.

• | Release the 5 clips (3).

• | Remove the hose for the windshield washer/wiper nozzle (2).

4. Remove the wiper system module.

• | Remove the 3 bolts (1).

• | Disconnect the wiring harness plug (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiper system module.

Tighten
Tighten the 3 bolts to 9 N·m (80 lb in).

2. Connect the wiring harness plug.
3. Install the windshield air inlet screen.

• | Install the hose for the windshield nozzle.

• | Install the 5 clips.

4. Install the windshield wiper arms.

| Important: Ensure correct installation position of the windshield wiper arms.

• | Place the 2 windshield wiper arms on the shaft.

• | Install the 2 washers.

Tighten
Tighten the 2 nuts to 17 N·m (13 lb ft).

• | Install the 2 covers.

5. Install the windshield trim seal.
6. Adjust the wiper arms. Refer to Windshield Wiper Arm Adjustment .