For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the water pump strap disc (1).

• | Remove the 3 bolts (2).

• | Do not remove.

• | Counterhold against the bolt of the torsional vibration damper.

3. Raise the vehicle by its full height.
4. Remove the drive belt. Refer to Drive Belt Replacement .
5. Drain the coolant.

• | Place a drain pan underneath.

• | Install the suitable hose to the drain connection (2).

• | Open the coolant drain screw (1).

• | Drain the coolant.

• | Close the coolant drain screw.

6. Lower the vehicle by its full height.
7. Remove the water pump strap disc.

Remove the 3 bolts.

8. Remove the water pump (2) from the pump module (1).

• | Remove the 5 bolts.

• | Remove the water pump.

9. Clean the sealing surfaces.
10. Clean the thread.

Clean the 3 water pump threads.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the water pump.

Use NEW bolts.

Tighten
Tighten the 5 bolts to 8 N·m (70 lb in).

2. Install the water pump strap disc.

• | Install the 3 bolts.

• | Use NEW bolts.

3. Raise the vehicle.
4. Install the drive belt. Refer to Drive Belt Replacement .
5. Lower the vehicle.
6. Install the water pump belt pulley.

Tighten
Tighten the 3 bolts to 20 N·m (15 lb ft).

7. Fill and bleed the cooling system. Refer to Cooling System Draining and Filling .
8. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .