For 1990-2009 cars

#### Special Tools

KM-498-B Oil Pressure Gage

### Removal Procedure

1. Open the hood.
2. Unscrew the closure bolt (1).
3. Clean the thread.

### Measurement Procedure

1. Attach KM-498-B (2) in combination with KM-232 (1).

2. Start the engine.
3. Oil Pressure, Check

At idling speed, the oil pressure must be at least 130 kPa (1.3 bar) and the oil temperature must be >=80°C.

### Installation Procedure

1. Switch off the engine.
2. Detach KM-498-B together with KM-232.

Notice: Refer to Fastener Notice in the Preface section.

3. Install new closure bolt in the cylinder head.

Tighten
Tighten bolt 15 N·m.

4. Check the engine oil level.
5. Close the hood.