For 1990-2009 cars

### Removal Procedure

1. Lower the window.
2. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the belt inner sealing strip.

Pull the channel strip carefully from behind beginning at the top.

### Installation Procedure

1. Install the belt inner sealing strip
2. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Close the window.