For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle by its full height.
2. Remove the engine front mount.

• | Remove the 2 bolts (1).

• | Remove the screwed connection (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine front mount.

Use new nuts.

Tighten

• | Tighten the screwed joint to 55 N·m (40 lb ft).

• | Tighten the 2 bolts to 80 N·m (59 lb ft).

2. Lower the vehicle.