For 1990-2009 cars

#### Special Tools

SA9211T-2 /KM-161-B and KM-161-2

### Removal Procedure

1. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
2. Measure the exposed thread length from the lock nut to thread end of the tie rod.
3. Release the lock nut (1).

Counterhold with open-ended wrench on the tie rod end.

4. Release the tie rod end from the steering knuckle.
5. Remove the tie rod end nut.
6. Press the tie rod end out of the steering knuckle using SA9211T-2 /KM-161-B and KM-161-2 (1).
7. Remove the tie rod end from the tie rod.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: First inspect exposed thread length.

1. Install the tie rod end to the tie rod.

Tighten
Tighten to 60 N·m (44 lb ft).

2. Lock the tie rod end with the lock nut.

Counterhold with an open-ended wrench on the tie rod end.

3. Install the tie rod end to the steering knuckle.

Tighten
Tighten the nut to 30 N·m (22 lb ft) plus 90 degrees, plus 15 degrees.

4. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
5. Inspect the toe-in, adjust if necessary. Refer to Front Toe Adjustment .