For 1990-2009 cars

### Removal Procedure

1. Remove the front side door panel.

Remove the access panel (1) with a plastic wedge.

Important: The moveable handle part must now be secured in pulled position.

2. Remove the fixed handle part of the front door with lock cylinder.

• | Pull out and hold the moveable handle part (I).

• | Turn the bolt (II) left until it stops.

• | Remove the fixed handle part with lock cylinder (III).

3. Remove the lock cylinder cover.

Remove the cover cap.

### Installation Procedure

1. Install the lock cylinder cover.

Clip the cover into position.

Important: Hold the moveable handle part in place while turning bolt.

2. Install the front door fixed handle part with lock cylinder.

• | Install the fixed handle part with the lock cylinder.

• | Turn the bolt right until it stops.

• | Insert the cover cap.

3. Install the front side door panel.