For 1990-2009 cars

## Headlamp Bulb Replacement without High Intensity

### Removal Procedure

Caution: Refer to Halogen Bulb Caution in the Preface section.

1. Open the access panel in the wheelhouse liner.
2. Remove the cover access on the headlamp.

Important: Release the lamp holder by twisting (arrow).

3. Remove the lamp holder.
4. Disconnect the lamp.

• | Release the 2 clips (1).

• | Disconnect the wiring harness plug (2).

### Installation Procedure

1. Connect the lamp.

Connect the wiring harness plug.

2. Install the lamp holder.

Important: Ensure correct position of the access panel.

3. Install the access cover on the headlamp.
4. Close the access panel in the wheelhouse liner.