For 1990-2009 cars

#### Special Tools

KM-6009 Remover/Installer

### Removal Procedure

1. Open the hood.
2. Remove the engine wiring trough (1) from the cylinder head.

Position the wiring trough to one side.

3. Disconnect the DIS-ignition module wiring harness plug (2).
4. Remove the DIS-ignition module.

| Note: Note the arrow on the cover.

• | Remove the cover of the DIS-ignition module in the direction of the arrow.

• | Remove the 2 bolts.

• | Remove from the spark plugs using KM-6009 (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: When installing a new DIS-ignition module it is not necessary to replace the gaskets.

1. Install the DIS-ignition module (1) with KM-6009 .

• | Replace the gaskets (2).

Tighten
Tighten the 2 bolts to 8 N·m (71 lb in).

• | Install the DIS-ignition module cover.

2. Connect the DIS-ignition module wiring harness plug.
3. Connect the engine wiring trough to cylinder head.
4. Close the hood.