For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.

Important: Remove the headlining in the vehicle interior.

2. Lower the headlining. Refer to Headlining Trim Panel Replacement .
3. Remove the object alarm speaker.

• | Disconnect the wiring harness plug (1).

• | Remove the speaker (2) from the headlining.

### Installation Procedure

1. Install the object alarm speaker.

• | Install the speaker to the headlining.

• | Connect the wiring harness plug.

2. Install the headlining. Refer to Headlining Trim Panel Replacement .
3. Connect the battery.
4. For reprogramming procedures, refer to Control Module References .