For 1990-2009 cars

### Removal Procedure

1. Open the sunroof.
2. Remove the sunroof air deflector covers from each side.

Release the cover (1) at the back (3) and remove from the front bracket (2).

3. Remove the wind deflector.

3.1. | Remove the wind deflector with the wind deflector swing-out arm.

3.2. | Remove the 2 screws (1).

3.3. | Remove the 5 wind deflector clamps (3).

3.4. | Slide the wind deflector rearward.

3.5. | Remove the bracket from the guide (2).

4. Remove the wind deflector swing-out arm.

Remove the screw (1) and the swing-out arm.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wind deflector swing-out arm.

Tighten
Tighten the bolt to 2 N·m (18 lb in).

2. Install the wind deflector.

2.1. | Insert the wind deflector into the side guide.

2.2. | Clamp the wind deflector.

2.3. | 5 clamps

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

3. Install the sunroof air deflector covers.

Insert and clip in the covers.

4. Close the sunroof.
5. Close the sunshade.