For 1990-2009 cars

### Removal Procedure

Note:

• | If replacing the instrument cluster, check which version of the fuel tank fuel level sensor is installed.

• | When replacing the control unit, before removing the control unit, carry out a Reset using a scan tool. For reprogramming procedures, refer to Control Module References.

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.

Disconnect the negative battery cable.

2. Remove the lower steering column paneling.

• | Remove the 5 bolts (arrows).

• | Remove the ignition lock panel (1).

3. Remove the instrument cluster.

• | Remove the 2 bolts (1).

• | Disconnect the wiring harness plug.

• | Release the wiring harness plug and disconnect.

• | Remove the instrument cluster (3) with the upper steering column paneling (2).

4. Remove the upper steering column paneling (1) from the instrument cluster (2).

### Installation Procedure

1. Install the upper steering column paneling to the instrument cluster.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the instrument cluster.

• | Insert the instrument cluster with the upper steering column paneling.

• | Connect the wiring harness plug.

Tighten
Tighten the 2 screws to 2.5 N·m (22 lb in).

3. Install the lower steering column paneling.

• | Fold down the upper steering column paneling.

Tighten
Tighten the 5 screws to 0.9 N·m (8 lb in).

• | Install the ignition lock panel.

• | Install the 2 screw head covers.

• | Insert knobs for the screen wiper switch and the indicator switch.

4. Connect the battery.

Connect the negative battery cable.

Note: If replacing the instrument cluster, check which version of the fuel tank fuel level sensor is installed.

5. For reprogramming procedures, refer to Control Module References.