For 1990-2009 cars

### Removal Procedure

1. Remove the upper extension trim panel.
2. Release the 3 clips.
3. Disconnect the wiring harness plug.
4. Remove the front door outer mirror.

4.1. | Disconnect the wiring harness plug.

4.2. | Remove the 3 bolts.

4.3. | Remove the outer mirror.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front door outer mirror.

Tighten
Tighten the 3 bolts to 5 N·m (44 lb in).

2. Connect the wiring harness plug.
3. Install the outer mirror inner paneling.
4. Connect the wiring harness plug.
5. Install the 3 clips.
6. Perform the operational inspection.