For 1990-2009 cars

### Removal Procedure

1. Remove the ball head (3) of the sensor linkage.
2. Remove the sensor.

• | Disconnect the wiring harness plug (1).

• | Remove the 2 bolts (2).

• | Remove the rear headlamp leveling sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear headlamp leveling sensor.

• | Insert the rear headlamp leveling sensor.

Tighten
Tighten the 2 screws to 5 N·m (44 lb in).

• | Connect the wiring harness plug.

2. Install the ball head for the sensor linkage.