For 1990-2009 cars

1. Install the rear planetary ring gear flange (605) into the rear planetary ring gear (606) in the direction as shown in the figure.
2. Install the rear planetary ring gear flange retaining ring (604) in the groove of the rear planetary ring gear.
3. Install the coast clutch outer race (607).

Note: Do not mistake the direction of the one way clutch.

4. Install the coast clutch end bearings (608) and the coast one way clutch (609).
5. Install the coast clutch retainer plate (610).
6. Install the coast clutch retainer plate retaining ring (611) with a screwdriver.
7. Install the rear planetary ring gear assembly to the overdrive clutch and coast clutch assembly.
8. Hold the clutch assembly and turn the rear planetary ring gear assembly. The rear planetary ring gear assembly should turn freely clockwise and should lock counterclockwise.