For 1990-2009 cars

### Removal Procedure

1. Remove the left front wheel and tire. Refer to Tire and Wheel Removal and Installation.
2. Remove the electrical connector at the input speed sensor.
3. Remove the retaining bolt (75) and the sensor (76).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the speed sensor (76) and the retaining bolt (75).

Tighten
Tighten the stud to 5 N·m (44 lb in).

2. Install the electrical connector at the sensor.
3. Install the left front wheel and tire. Refer to Tire and Wheel Removal and Installation.