For 1990-2009 cars

## Rear Bumper Fascia Outer Support Replacement Coupe

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the outer supports.

Drill out the 6 blind rivets (arrows).

3. Remove the outer supports.

### Installation Procedure

1. Prepare the outer supports.
2. Install the outer supports.

Rivet on the 6 blind rivets.

3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .

## Rear Bumper Fascia Outer Support Replacement Sedan

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the fascia outer support.

Drill out the 6 blind rivets (arrows).

3. Remove the fascia outer support.

### Installation Procedure

1. Prepare the fascia outer support.
2. Install the fascia outer support.

Rivet on the 6 blind rivets.

3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .