For 1990-2009 cars

## Rear Compartment Sill Trim Plate Replacement Sedan

### Removal Procedure

• |
- Remove the rear compartment sill trim plate.

• |
- Remove carefully in the upper area (2) with a plastic wedge.

• |
- Release the 4 clips.

• |
- Release in the lower area (1) in the direction of the interior.

• |
- Release the 4 clips.

### Installation Procedure

• |
- Install the rear compartment sill trim plate.

• |
- Install the 8 clips.

## Rear Compartment Sill Trim Plate Replacement Coupe

### Removal Procedure

1. Remove the rear compartment carpet.
2. Remove the trailer hitch ball head.

• | Loosen the fastening belt (1).

• | Remove the ball head (2).

3. Remove the additional storage tray under the load compartment carpet.
4. Remove the rear compartment sill trim plate.

Release the 7 clips (1).

### Installation Procedure

1. Install the rear compartment sill trim plate.

Install the 7 clips.

2. Install the additional storage trays under the load compartment carpet.
3. Install the trailer hitch ball head.

• | Thread the belt through the eye.

• | Insert the ball.

• | Tighten the belt.

4. Install the rear compartment carpet.