For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Bracket Bolt | 5 N·m | 44 lb in
Battery Holder Bolt | 15 N·m | 11 lb ft
Battery Negative Connection Nut | 5 N·m | 44 lb in
Condenser to Radiator Bolts | 5 N·m | 44 lb in
Coolant Pump Manifold Bolts | 8 N·m | 71 lb in
Exhaust Camshaft Adjuster | 65 N·m | 48 lb ft
Plus 120 Degrees Plus 15 Degrees
Exhaust Camshaft Adjuster Closure Bolt | 30 N·m | 22 lb ft
Fan Housing to Radiator Bolts | 5 N·m | 44 lb in
Fan Motor to Fan Housing Bolts | 3 N·m | 26 lb in
Front Fascia Bolts - Bottom | 2.5 N·m | 22 lb in
Front Fascia Bolts - Top | 2.5 N·m | 22 lb in
Ground Connection to Ground Terminal Nut | 5 N·m | 44 lb in
Heat Exchanger to Oil Filter Adapter Bolts | 2.5 N·m | 22 lb in
Intake Camshaft Adjuster | 65 N·m | 48 lb ft
Plus 120 Degrees Plus 15 Degrees
Intake Camshaft Adjuster Closure Bolt | 30 N·m | 22 lb ft
Negative Connection to Ground Terminal Nut | 5 N·m | 44 lb in
Oil Cooling Line Bolt - Lower | 25 N·m | 18 lb ft
Oil Cooling Line Bolt - Upper | 25 N·m | 18 lb ft
Oil Filter Adaptor Bolts | 8 N·m | 71 lb in
Positive Cable to Positive Terminal Bolt | 5 N·m | 44 lb in
Positive Connection to Positive Terminal Nut | 5 N·m | 44 lb in
Radiator Bracket Bolts - Bottom of Radiator | 5 N·m | 44 lb in
Radiator Bracket Bolts - Lower | 15 N·m | 11 lb ft
Rear Toothed Belt Cover Bolts | 6 N·m | 53 lb in
Thermostat Housing Bolts | 8 N·m | 71 lb in
Thermostat Housing Coolant Pipe to Oil Filter Adapter Bolts | 8 N·m | 71 lb in
Water Pump Belt Pulley Bolts | 20 N·m | 15 lb ft
Water Pump Bolts | 8 N·m | 71 lb in
Wiring Harness Bracket Nut | 2.5 N·m | 22 lb in
Wiring Harness Bracket to Thermostat Housing Nut | 5 N·m | 44 lb in