For 1990-2009 cars

### Removal Procedure

Important:

• | The fuel tank must be drained with a suitable, commercially-available fuel removal unit and suction hose - follow safety regulations and national legislation. The fuel tank is fitted with a refill limit float valve. This is located on the filler neck in the fuel tank. To prevent damaging the refill limit float valve, a suitable suction hose must be used.

• | In the presence of fuel vapors or escaping fuel - observe safety regulations and national legislation. Store drained fuel in a suitable, sealable container.

1. Remove the fuel tank. Refer to Fuel Tank Replacement .

Important: Do not pull on the shaft of fuel tank sensor.

2. Remove the fuel tank sensor (1).

• | Release the 2 retainers (3).

• | Carefully pull from guide upward .

| Important: The wire connectors are to be pulled out carefully for disassembling of the connection wires.

• | Disconnect the 2 wires.

| Important: The cable connectors is to be depressed by a blunt rod-shaped article.

• | Depress the 2 snap-on tongue (arrows) of the cable connectors .

### Installation Procedure

Important: Do not pull on shaft of fuel tank sensor.

1. Install the fuel tank sensor.

• | Lock the 2 retainers .

• | Carefully pull in guide downward.

| Important: The wire connectors are to be pulled in carefully for disassembling of the connection wires.

• | Connect the 2 wires.

2. Install the fuel tank. Refer to Fuel Tank Replacement .