For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. For vehicles with high-pressure headlamp washer hose, remove the high-pressure headlamp washer hose (1) from the front panelling grille guide.
3. Remove the front lower fascia grille.

Remove the 20 retainers (arrows).

### Installation Procedure

1. Install the front lower fascia grille.

Insert and lock the 20 retainers.

2. For vehicles with high-pressure headlamp washers, install the high-pressure headlamp washer hose in the front panelling grille guide.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .