For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.
2. Deactivation of the airbag discharge time capacitor.
3. Position the seat to the most forward position.
4. Remove the front seat belt fastening panel.

Remove the panel upwards (1).

5. Remove the seat belt from the front seat.

Remove the bolt (2).

6. Remove the driver seat, rear.

Remove the 2 bolts (1).

7. Remove the front seat.

• | Remove from the front guide.

• | Release and disconnect the compact connector.

### Installation Procedure

1. Install the front seat.

• | Connect and latch the compact connector.

• | Insert the seat in the front guide.

Caution: Refer to Fastener Caution in the Preface section.

Note: Use screw locking compound.

2. Fasten the front seat.

Tighten
Tighten the 2 bolts to 35 N·m (26 lb ft).

Note: Use screw locking compound.

3. Install the front seat, seat belt.

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

Note: Use screw locking compound.

4. Insert the front seat, seat panel.

Reposition the front seat to the original position.

5. Connect the battery.
6. For programming procedures, refer to Control Module References.