For 1990-2009 cars

### Removal Procedure

Remove the instrument panel (I/P) compartment.

1. Open the I/P compartment door.
2. Remove the 4 bolts (1).
3. Disconnect the wiring harness plug.
4. Remove the I/P compartment.

### Installation Procedure

1. Insert the I/P compartment.

Connect the wiring harness plug.

Notice: Refer to Fastener Notice in the Preface section.

2. Fasten the I/P compartment.

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).

3. Close the glove compartment door.