For 1990-2009 cars

### Removal Procedure

1. Remove the radio.

• | Install the removal bar into the openings (arrows) until it engages.

• | Pull both removal bars outwards and at the same time withdraw the radio from the holder.

2. Disconnect the wiring harness plug.

Disconnect the 2 wiring harness plugs (1, 2).

3. Disconnect the radio storage frame (arrows) and remove.

### Installation Procedure

1. Install the radio storage frame.
2. Connect the 2 wiring harness plugs.
3. Install the radio.

Push the radio into the holder until it audibly engages.

4. Program the radio.