For 1990-2009 cars

## Liftgate Garnish Molding Replacement Sedan

### Removal Procedure

1. Remove the upper liftgate garnish molding--left side.

• | Remove the luggage shade bracket.

• | Release the 4 clips.

2. Remove the upper liftgate garnish molding--right side.

• | Remove the luggage shade bracket.

• | Release the 4 clips.

### Installation Procedure

1. Install the upper liftgate garnish molding--right side.

• | Install the 4 clips.

• | Tighten the luggage shade bracket.

2. Install the upper liftgate garnish molding--left side.

• | Install the 4 clips.

• | Tighten the luggage shade bracket.

## Liftgate Garnish Molding Replacement Coupe

### Removal Procedure

1. Support the luggage shade from the liftgate.

Disconnect the 2 retaining cords.

2. Remove the upper right and the left liftgate garnish molding (1).

• | Remove the 2 luggage shade retainers (2).

• | Release the 6 clips.

### Installation Procedure

1. Install the upper right and the left liftgate garnish molding.

• | Install the 6 clips.

• | Install the 2 luggage shade retainers.

2. Support the luggage shade to the liftgate.

Attach the 2 retaining cords.