For 1990-2009 cars

1. Clean the sealing surfaces and the 3 coolant pump threads.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the coolant pump (2) and 5 NEW bolts.

Tighten
Tighten the bolts to 8 N·m (71 lb in).

3. Install the coolant pump strap disc and 3 NEW bolts.
4. Install the ribbed V-belt.
5. Attach the coolant pump belt pulley.

Tighten
Tighten the 3 bolts to 20 N·m (15 lb ft).

6. Fill and bleed the cooling system.
7. Install the air cleaner housing.