For 1990-2009 cars

### Removal Procedure

1. Remove the bench seat.

1.1. | Unlock the 2 front brackets (1).

1.2. | Support the 2 bench seats from the rear bracket.

1.3. | Push the seat simultaneously backwards and upward.

2. Remove the rear seat back.

2.1. | Remove the 3 bolts at the front and remove the belt buckles.

2.2. | Fold down the rear seat back.

2.3. | Remove the 3 bolts at the back.

3. With the aid of an assistant, remove the rear seat back.

Remove the rear seat back from the side guide.

### Installation Procedure

1. With the aid of an assistant, insert the rear seat back, insert the rear seat back into the side guide.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear seat back.

Tighten
Tighten the 3 rear bolts to 20 N·m (15 lb ft).

Important: Use screw locking compound

3. Fold down the rear seat backrest.

Tighten
Tighten the front 3 bolts to seat belt buckle to 20 N·m (15 lb ft).

4. Install the rear seat.

Insert the rear seat cushion and position.