For 1990-2009 cars

Table 1: | Transmission Clearance Specifications
Table 2: | Clutch Assembly Specifications

#### Transmission Clearance Specifications

Application | Specification
--- | ---
Metric | English
Front Differential Assembly (13)

- Unloaded Rotating Torque - New Bearings

0.78-1.37 N·m

7-12 lb in

- Unloaded Rotating Torque - Reused Bearings

0.39-0.69 N·m

3-6 lb in

Fluid Pump Assembly (2)

- Driven Gear (189) to Body Clearance - Maximum

0.15 mm

0.006 in

- Drive Gear (190) Tip to Body Clearance - Maximum

0.25 mm

0.010 in

- Driven Gear (189) Tip to Body Clearance - Maximum

0.25 mm

0.010 in

- Fluid Pump Body Bushing, ID - Maximum

38.138 mm

1.500 in

- Side Clearance of Drive and Driven Gear to Body

0.02-0.05 mm

0.0008-0.0020 in

- Stator Shaft Bushing, ID - Maximum

18.026 mm

0.710 in

2nd and 4th Gear Band Servo (56)

- Piston Stroke

2.659-3.141 mm

0.105-0.123 in

#### Clutch Assembly Specifications

Application | Specification
--- | ---
Metric | English
Overdrive Clutch - C0 (15)

- Piston Stroke

1.043-1.357 mm

0.041-0.053 in

- Relaxed Clutch Pack Stack Up Clearance

0.341-0.979 mm

0.013-0.039 in

- Available Overdirive Clutch Backing Plate (210) Thickness

3.6 mm

0.142 in

3.8 mm | 0.150 in
4.0 mm | 0.157 in
Forward Clutch - C1 (18)

- Piston Stroke

0.442-0.758 mm

0.017-0.030 in

- Relaxed Clutch Pack Stack Up Clearance

0.442-0.758 mm

0.017-0.030 in

- Available Forward Clutch Backing Plate (576) Thickness

3.4 mm

0.134 in

3.6 mm | 0.142 in
3.8 mm | 0.150 in
1st and Reverse Clutch (B2)

- Piston Stroke

1.730-2.570 mm

0.068-0.10 in

- Relaxed Clutch Pack Stack Up Clearance

0.599-1.901 mm

0.024-0.075 in

Reverse Clutch - C2 (23)

- Piston Stroke

0.932-1.608 mm

0.367-0.0633 in

- Relaxed Clutch Pack Stack Up Clearance

0.432-1.228 mm

0.017-0.048 in

Coast Clutch - C3 (15)

- Piston Stroke

2.682-3.018 mm

0.106-0.12 in

- Relaxed Clutch Pack Stack Up Clearance

2.211-2.769 mm

0.087-0.109 in