For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle all the way.
2. Release the muffler fastening clamp.

Remove the nut (1).

3. Remove the muffler from the bracket (1) in 2 places.

Note: Slider.

4. Remove the muffler from the mid muffler.
5. Clean the sealing surface.

### Installation Procedure

1. Install the muffler to the mid muffler.
2. Insert the muffler in the bracket in 2 places.
3. Align the exhaust system.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the muffler fastening clamp.

Tighten
Tighten the nut 50 N·m (37 lb ft).

5. Lower the vehicle all the way.