For 1990-2009 cars

#### Special Tools

J 39637 /KM-6626 Wiper Arm Puller

### Removal Procedure

Remove the wiper arm.

• | Open the cover.

• | Remove the nut.

• | Pull off the wiper arm using J 39637 /KM-6626.

### Installation Procedure

Install the rear wiper arm.

• | Extend the wiper arm.

Notice: Refer to Fastener Notice in the Preface section.

• | Align the wiper arm parallel to the bottom edge of the liftgate window.

Tighten
Tighten the nut to 9 N·m (80 lb in).

• | Close the cover.