For 1990-2009 cars

#### Special Tools

• | KM-446 Installer Drift

• | KM-557-A Remover

### Removal Procedure

1. Remove the axle shaft affected from transmission. Refer to Wheel Drive Shaft Replacement .

Important: Place a drip pan underneath, transmission fluid will escape. Axle shaft remains in wheel hub.

2. Remove the affected axle shaft seal ring with KM-557-A (2) and KM-446 (1) from transmission housing.

### Installation Procedure

1. Install the new axle shaft seal ring.

• | Coat the axle shaft seal ring with transmission fluid.

• | Install the axle shaft seal ring flush in the transmission. For F17 use KM-446 (1)

2. Install the axle shaft in the transmission. Refer to Wheel Drive Shaft Replacement .
3. Inspect the transmission fluid level. Refer to Transmission Fluid Check .