For 1990-2009 cars

### Removal Procedure

1. Remove the hand brake molding (1).

Disconnect the hand brake molding.

2. Remove the ashtray.

2.1. | Disconnect the 2 wiring harness plugs.

2.2. | Remove the ashtray.

3. Remove the shift level bezel.

Remove the 2 bolts (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the shift level bezel.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

2. Install the ashtray.

2.1. | Insert the ashtray.

2.2. | Connect the 2 wiring harness plugs.

3. Install the hand brake molding.

Connect the hand brake molding.