For 1990-2009 cars

## Communication Interface Module Replacement Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove Instrument Panel Compartment. Refer to Instrument Panel Compartment Replacement.

1 | Communication Interface Module Bolt (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 4 N·m (35 lb in)
2 | Communication Interface Module Battery
3 | Communication Interface Module Bracket
4 | Communication Interface Module

#### Procedure

1. Disconnect the electrical connections.
2. Refer to Control Module References for programming and set up procedures.

## Communication Interface Module Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the driver knee bolster. Refer to Driver Knee Bolster Replacement.

1 | Communication Interface Module Bolt (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 4 N·m (35 lb in)
2 | Communication Interface Module

#### Procedure

1. Disconnect the electrical connections.
2. Refer to Control Module References for programming and set up procedures.

3 | Communication Interface Module Bolt (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 4 N·m (35 lb in)
4 | Mobile Telephone Transceiver