For 1990-2009 cars

### Removal Procedure

1. Release the windshield outside moisture sensor cover (1).
2. Remove the windshield outside moisture sensor.

• | Disconnect the wiring harness plug (2).

• | Release the 2 clamps (3).

### Installation Procedure

1. Install the windshield outside moisture sensor.

• | Connect the wiring harness plug.

• | Close the 2 clamps.

2. Install the windshield outside moisture sensor cover.