For 1990-2009 cars

## Cargo Lamp Replacement Sedan

### Removal Procedure

1. Remove the cargo lamp.

• | Release using a suitable tool (plastic wedge).

• | Disconnect the wiring harness plug (1).

2. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Install the cargo lamp.

• | Connect the wiring harness plug.

• | Install the lamp.

## Cargo Lamp Replacement Coupe

### Removal Procedure

1. Open the liftgate.
2. Remove the cargo lamp.

• | Release the lamp.

• | Disconnect the wiring harness plug (1).

• | Remove the bulb.

### Installation Procedure

1. Install the cargo lamp.

• | Insert the lamp.

• | Connect the wiring harness plug.

• | Install the cargo lamp.

2. Close the liftgate.