For 1990-2009 cars

### Removal Procedure

1. Remove the bench seat.

1.1. | Unlock the 2 brackets (1) front.

1.2. | Support 2 bench seats from the rear bracket.

1.3. | Push the seat simultaneously backwards and upward.

2. Remove the center rear seat backrest.

2.1. | Remove the 2 bolts at the front and remove the belt buckle.

2.2. | Remove the 4 bolts, side.

2.3. | Fold down the rear seat backrest.

2.4. | Remove the 2 bolts at the back.

3. Remove the head restraints.
4. Remove the head restraint guide sleeve.

Remove the 2 head restraint guide sleeves with a suitable tool.

5. Remove the rear seat backrest cover.

Remove the 11 clips.

6. Remove the brackets, right and left.

Remove the 2 bolts.

7. Remove the lock panel.

Remove the 2 bolts (1).

8. Remove the cushion cover.

Remove the cushion cover all the way around.

### Installation Procedure

1. Install the cushion cover.

Position the cushion cover.

2. Insert surrounding cushion cover.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lock panel.

Tighten
Tighten the 2 bolts to 25 N·m (18 lb ft).

4. Install the head restraint guide sleeve.

Engage the 2 head restraint guide sleeves (audible click).

5. Install the brackets, right and left.

Tighten
Tighten the 2 bolts to 25 N·m (18 lb ft).

6. Install the rear seat backrest cover.

Install the 11 clips.

7. Install the head restraints.
8. Insert the rear seat backrest.

Important: Use screw locking compound.

9. Install the rear seat backrest.

Tighten
Tighten the 2 screws at back to 20 N·m (15 lb ft).

Important: Use screw locking compound.

10. Fold down the rear seat backrest.

Insert the seat belt buckle.

Tighten

• | Tighten the 4 bolts to 20 N·m (15 lb ft).

• | Tighten the 2 front bolts to 20 N·m (15 lb ft).

11. Insert the rear seat cushions and lock.