For 1990-2009 cars

### Removal Procedure

Important: The wiper switch is replaced in a similar manner.

Remove the actuating lever.

1. Pull the rubber sleeve out of the steering column paneling.

Important: Unlock the engaging lug with a suitable tool (1), a hex screwdriver 1.5 mm WAF.

2. Release the retaining lug.
3. Remove the multifunction switch.

### Installation Procedure

Install the multifunction switch.

1. Engage the multifunction switch.
2. Install the rubber sleeve in the steering column paneling.