For 1990-2009 cars

### Removal Procedure

1. Open the access panel.
2. Remove the tail lamp.

• | Remove the 2 wing nuts (1).

• | Disconnect the wiring harness plug (2).

3. Remove the tail lamp holder.

Release the 3 tail lamp holders (3).

4. Remove the bulb.

### Installation Procedure

1. Insert the bulb.
2. Install the lamp holder.

Clip the bulb holder in position.

Important:

• | Before fitting the tail lamp, ensure that the tail lamp gasket is seated correctly.

• | Note the gaskets (2, 3) fit only in the intended positions due to their shape.

3. Install the gasket (1).
4. Install the tail lamp.
5. Connect the wiring harness plug.

Tighten the 2 wing nuts.

6. Close the access panel.