For 1990-2009 cars

The following services should be performed at the first maintenance service (I or II) after the indicated miles (kilometers) shown for each item.

#### Additional Required Services

Service and Miles (Kilometers) | 25,000 (40 000) | 50,000 (80 000) | 75,000 (120 000) | 100,000 (160 000) | 125,000 (200 000) | 150,000 (240 000)
--- | --- | --- | --- | --- | --- | ---
Inspect fuel system for damage or leaks. | · | · | · | · | · | ·
Inspect exhaust system for loose or damaged components. | · | · | · | · | · | ·
Replace engine air cleaner filter. See "Engine Air Cleaner/Filter" in the owner manual. |  | · |  | · |  | ·
Replace passenger compartment air filter. | · | · | · | · | · | ·
Change automatic transmission fluid (severe service). See footnote (i). |  | · |  | · |  | ·
Change automatic transmission fluid (normal service). |  |  |  | · |  |
Replace spark plugs. An Emission Control Service. Not to exceed 35,000 miles (56 000 km). | · | · | · | · | · | ·
Engine cooling system service (or every five years, whichever occurs first). An Emission Control Service. See footnote (j). |  |  |  |  |  | ·
Solid lifter tappet adjustment (or every 10 years, whichever occurs first). See footnote (m). Not to exceed 90,000 miles (144 000 km). |  |  | · |  |  | ·
Replace timing belt and tensioner (or every 10 years, whichever occurs first). See footnote (m). Not to exceed 100,000 miles (160 000 km). |  |  | · |  |  | ·
Inspect engine accessory drive belt (or every two years, whichever occurs first). An Emission Control Service. See footnote (k). Not to exceed 36,000 miles (58 000 km). | · | · | · | · | · | ·
Change brake and clutch hydraulic fluid at a regular maintenance service every two years. See footnote (l). |  |  |  |  |  |