For 1990-2009 cars

Condition | Action
--- | ---
The pivot bolt is damaged or misaligned. | Replace or properly align the pivot bolt.
The tilt lever assembly adjustment nut is too tight. | Loosen the tilt lever assembly adjustment nut and adjust the lever until tilt effort is correct.
The tilt lever assembly or the tilt teeth are damaged. | If necessary, replace the steering column. Refer to Steering Column Replacement .