For 1990-2009 cars

1. Remove the 2 fluid pump cover O-ring seals (193).

Note: Be careful not to drop the fluid pump body.

2. Loosen the 8 fluid pump cover bolts (192) and remove the fluid pump cover and stator shaft assembly (191).

Note: If the drive gear and driven gear have any damage, replace them.

3. Remove the fluid pump body driven gear (189) and fluid pump body drive gear (190) from the fluid pump body (187).
4. Remove the fluid pump body seal assembly (186).