For 1990-2009 cars

### Removal Procedure

1. Disconnect the wiring harness plug for pressure sensor (1).

Release and disconnect the wiring harness plug.

2. Remove the pressure sensor (2).

### Installation Procedure

1. Install the pressure sensor.

Caution: Refer to Fastener Caution in the Preface section.

2. Replace the seal ring.

Tighten
Tighten the pressure sensor to 10 N·m (89 lb in).

3. Connect the wiring harness plug.