For 1990-2009 cars

## Front Side Door Window Channel Replacement Sedan

### Removal Procedure

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Partly loosen water vapor barrier.

• | Remove the 2 front door retainer base inner panel.

• | Loosen the water vapor barrier in the area of the hatching.

3. Drill out the window channel.

Drill out the 2 rivets.

4. Remove the window channel.

### Installation Procedure

Important: Observe installation direction.

1. Install the rear front door window channel.

• | Rivet on 2 rivets.

• | Position in lower guide rail.

2. Install the water vapor barrier.

Install the 2 front door retainer base inner panel.

3. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .

## Front Side Door Window Channel Replacement Coupe

### Removal Procedure

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Lower the window.
2. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Partly loosen the water vapor barrier.

• | Remove the 2 holding angles.

• | Remove the 2 pins.

Important: Remove the window channel weatherstrip from inside with the appropriate tool.

4. Remove the outer belt sealing strip

• | Remove the window channel weatherstrip from the rear window frame bracket.

• | Remove the fastening clip from the outer window frames.

5. Remove the rear window channel.

Drill out the 2 blind rivets.

6. Remove the rear window channel.

### Installation Procedure

1. Position the rear window channel.
2. Install the rear window channel.

Rivet on 2 blind rivets.

3. Install the outer belt sealing strip.

• | Install the fastening clip on the outer window frame.

• | Install the window channel weatherstrip in the window channel bracket.

• | Install the window belt sealing strip onto the door folding.

4. Fasten the water vapor barrier.

• | Install the 2 holding angles.

• | Install the 2 pins.

5. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
6. Close the window.