For 1990-2009 cars

### Removal Procedure

1. Remove the front door emblem.

Carefully remove emblem with a plastic wedge (1).

Important: Ensure that the paint is not damaged.

2. Remove the remaining glue.

Remove the remaining glue from the door with a molding adhesive remover disk (2).

### Installation Procedure

1. Front door emblem dimensions are as follows:

• | Front clearance

• | Horizontal Vertical

• | I II

• | 125 mm (4.9 in) 150 mm (5.9 in)

2. Remove the protective strips from the emblem.
3. Install the front door emblem.

Align and glue on the front door emblem.