For 1990-2009 cars

### Removal Procedure

1. Remove the heating/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.
2. Remove the accessory panel from the instrument panel (I/P).

2.1. | Remove the 2 bolts (1).

2.2. | Release the panel.

2.3. | Disconnect the wiring harness plug (2).

2.4. | Release and disconnect wiring harness plug.

3. Remove the center air outlet (1).

Release the 6 clips (2).

### Installation Procedure

1. Install the center air outlet.

Install the 6 clips.

2. Install the accessory panel onto the I/P.

Caution: Refer to Fastener Caution in the Preface section.

3. Connect the wiring harness plug.

Clip in the panel.

Tighten
Tighten the 2 bolts to 5 N·m (44 lb in).

4. Install the heating/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.