For 1990-2009 cars

1. Install the NEW 2 transmission fluid passage seals (89) and 1 transmission fluid passage seal (85).
2. Remove any gasket material and be careful that no oil is on the contacting surfaces of the torque converter housing (10).
3. Apply a 3 mm (1/8 in) bead of sealant GM P/N 89020326 (Canadian P/N 89021188) to the torque converter housing as shown.
4. Install the torque converter housing (10).
5. Install thread locker GM P/N 12345382 (Canadian P/N 10953489) on the torque converter bolts (801, 802, 813).

Notice: Refer to Fastener Notice in the Preface section.

6. Install the 15 torque converter bolts (801, 802, 813).

Tighten
Tighten bolts to 30 N·m (22 lb ft).