For 1990-2009 cars

#### Special Tools

• | KM-6333 Fixing Rod

• | MK-6340 Locking Tool

• | KM-6625 Flywheel Locking Device

1. prepare the right half of the MK-6340 for use on the Z 18 16 XER engines

| Important: The front panel of the MK-6340 -Right is recognized by the lettering "Right", arrow.

1.1. | Remove the front panel (1) from the MK-6340 -Right.

1.2. | Remove the 2 bolts (2).

Important:

• | The spot-type marking (4) on the intake camshaft adjuster does not correspond to the groove of the MK-6340 -Left during this process but must be somewhat above.

• | The spot-type marking (3) on the exhaust camshaft adjuster must correspond to the groove on the MK-6340 -Right.

2. Insert MK-6340 -Left (1) and MK-6340 -Right (2) into the camshaft adjuster.
3. Block the crankshaft.
4. Attach the KM-6625 .

4.1. | Detach the screwed connection (1).

4.2. | Insert the KM-6625 (2).

4.3. | Tighten the screwed connection (3).

5. Using an Allen key (1), apply tension to the timing belt tensioner (2) in the direction of the arrow. Fix, using the KM-6333 .
6. Mark the timing belt direction of rotation.
7. Remove the timing belt tensioner bolt (2).
8. Remove the timing belt tensioner (1).