For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ballast Bolts | 2.5 N·m | 22 lb in
Fog Lamp Screws | 2.5 N·m | 22 lb in
Ground Connection Nut | 5 N·m | 44 lb in
Headlamp Bolts | 2.5 N·m | 22 lb in
Headlamp Connector Bolts | 2.5 N·m | 22 lb in
Headlamp Control Module Bolts | 2.5 N·m | 22 lb in
Headlamp Front Paneling Bolts - Left Side | 2.5 N·m | 22 lb in
Headlamp Leveling Module Bolt/Nut | 2.5 N·m | 22 lb in
Headlamp Leveling Rear Suspension Height Sensor Screws | 5 N·m | 44 lb in
Interior Lamp Holder Screws - Front | 1.5 N·m | 13 lb in
Tail Lamp Circuit Board Screws | 5 N·m | 44 lb in
Xenon Lamp Cover Bolts | 2.5 N·m | 22 lb in