For 1990-2009 cars

#### Special Tools

KM-6157 Assembly Sleeves

### Removal Procedure

Important: Central release and release bearing are one part. Overhauling is not required. If damaged or leaky, replace entire central release.

1. Remove the transmission. Refer to Transmission Replacement .
2. Remove the pressure line (1).

Remove the union nut.

3. Remove the central release.

Remove the 3 bolts (arrow).

Important: Replace damaged components.

4. Inspect the seal ring (1) on the central release for damage.

### Installation Procedure

1. Clean the 3 threads (1) in the transmission.

Notice: Refer to Fastener Notice in the Preface section.

Important: It is essential to avoid pulling the central release at an angle.

2. Install the central release (1).

| Important: Check the seal ring (arrow) for damage.

• | Attach the assembly aid (3) to the drive shaft (2) with KM-6157 .

• | Lightly coat the seal ring in the central release with transmission fluid.

| Important: Use new bolts.

• | Install the 3 bolts evenly in contact with the flange.

Tighten
Tighten the 3 bolts to 5 N·m (44 lb in).

3. Install the pressure line (1).

Tighten
Tighten the retaining nut to 14 N·m (124 lb in).

4. Install the transmission. Refer to Transmission Replacement .